{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":5,"n_cols":4,"rows_kept":5,"merged":[[0,0,0,3],[2,0,3,0],[2,1,3,1]],"flags":["formulas_cached_only"]}
["设备重要参数对比表"]
["序号","设备名称","采购人拟定的需求参数","供应商拟提供产品对应的参数"]
[15,"有创呼吸机","▲5、开关机按键和旋转编码器需在屏幕正面两侧。"]
[null,null,"▲6、有创通气模式至少包含：容量控制通气下的辅助控制通气A/C和同步间歇指令通气SIMV（容量模式流速波形可调方波、50%和100%递减波）、压力控制通气下的辅助控制通气A/C和同步间歇指令通气SIMV、持续气道正压通气和压力支持CPAP/PSV、双相气道正压通气、压力调节容量控制通气及其压力调节容量控制同步间歇指令通气SIMV、气道压力释放通气APRV、自适应支持通气AMV（或ASV等以Otis公式最小呼吸功为通气目标的智能通气模式）、容量支持通气VS、无创通气和高流量氧疗模式，其中氧疗模式流速≥80L/min，"]
["……","……","……"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}